|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **SERVICE/PRODUCT** | **DETAILED DESCRIPTION** | **COST IN KSH** |  |
|  |  |  |  |  |
| 1. | Water Wells/Borehole Drilling (standard or expected drilling height is 40 feet(13.3 meters) | * Site visit
* Water identification area
* 50% deposit
* 35% payable After fortnight(2 weeks)
* 15% payable on work completion
* Extra feet above 40ft (starting from 41) chargeable at the rate of 1000ksh. Per feet.)
* Charges exclude stone crashing if encountered in the process of drilling.
* Charges exclude constructing and putting electrical or manual pump at the top of the well.
* Duration of drilling is one month if everything considered constant .i.e. the place is not too rocky.
* Accommodation and meals will be agreed upon before the work starts.
* Protecting the area surrounding the well is the duty of the owner after completion.
 | 60,000 |  |
| 2. | Trading in various type of tanks | * Silos water tanks.
* Plastic water tanks.
* Galvanized water tanks.
* Corrugated water tanks.
* Steel water tanks.
* Ferro cement above and underground water Tanks.
* Collapsible water tanks.
* The prices of the tanks depends on :-
* Type of the tank.
* Tank capacity.
* Transportation cost to the site.
* 100% to be paid up front.
 | As low as ksh.1,000 |  |
| 3. | Water Tanks cleaning services | * Site visit to establish where the Tank is and if plumbing services will be needed to unfix and fix back the tank.
* Charges depend on Tank Capacity.
* Deposit of 75% to be paid up front.
* 25% to be paid on work completion.
 | 0.50 ksh. Per liter |  |
| 4. | Water Tank Repair Services | * Site visit to establish the tank problem.
* Quotation given to the client prior to repair.
* 75% deposit paid up front.
* 25% paid on work completion.
 | As from Ksh. 1,000 |  |
| 5. | Water pans and Dams | * Depends on capacity required in cubic meters.
* All materials to be used are to be purchased by the client or the company on behalf of the client.
* If the client is purchasing the materials he/she should buy the correct and up to-standard materials as directed by the company.
* 80% deposit should be paid upfront and the rest on work completion.
* The company can construct the pans in stages if the client does not have sufficient funds (Using pan upgrading method.)
* The client will be liable on protection measures around the pan as it is considered a water body.
 | AS from ksh.10,000 |  |
| 6. | Water pumps, manual, solar, petrol, diesel and electric. | * Prices depend on which type and how many horsepower one needs.
* We charge installation fees after a site visit and give quote.
* All other components for fixing the pump can be purchased by the client with direction of the company or the company can buy on behalf of the client.
* 85% is paid upfront and the remaining 15% paid on delivery/work finished.
 | As from ksh. 5,000 |  |
| 7. | Water pumps Servicing | * Site visit to establish the problem
* We give quotation for the work to be done.
* 75% to be paid upfront before work starts.
* 25% to be paid on work completion.
 |  |  |
| 8. | Water gutters  | * We sell plastic gutters and their components.
* Prices depend on the length and components.
* We offer installation services.
* Installation depends on quote given after a site visit.
* 80% is paid upfront and 20 % paid on completion
 | As from ksh.3,000 |  |
| 9. | Water gutters Repair and replacement Services. | * Site visit to establish the gutter problem.
* Quotation given to the client prior to repair.
* 75% deposit paid up front.
* 25% paid on work completion
 | As from ksh.2000 |  |
| 10. | Water gutters cleaning services | * Site visit to establish where the gutter is and if plumbing services will be needed to unfix and fix back the tank.
* Charges depend on gutter length.
* Deposit of 75% to be paid up front.
* 25% to be paid on work completion.
 | Ksh.35 per feet. |  |
| 11. | House/Building plumbing services | * Site visit.
* Work quotation.
* Materials purchase.
* Installation.
* 75% paid as deposit.
* 25% paid on work completion.
 | Depends on the site, and materials. |  |
| 12. | Water Testing | * Duration 5 working days after submission of water samples.
 | As from ksh.5,000 |  |
| 13. | Water Education | * Done in school, open air meetings and any other gatherings of water industry
* Training is free
* Charges are on meals, transportation and accommodation where applicable.
 | As from ksh. 1,000 |  |
| 14. | Reviving Stalled water projects in Kisumu county | * Conversant with the history of the project.
* Revive the project through looking for funds or making it a private entity as the structures are still available.
 |  |  |